2.  A transmission tower is held by three guy wires anchored by bolts at B, C, and D. If the tension in wire AD is 315 lb, deter-mine the components of the force exerted by the wire on the bolt at D.