At t = 0 the switch S is closed with the capacitor uncharged. If C = 50 mF, e = 20 V, and R = 4.0 kW, what is the charge on the capacitor when I = 2.0 mA?