A p-V diagram for a standard Diesel cycle is shown below;



Formula;

 $η\_{l }$= 1 - $\frac{\left(T\_{4}-T\_{1}\right)}{γ\left(T\_{3}-T\_{2}\right)}$